***Annexure 1***

**Quotation**

|  |  |  |
| --- | --- | --- |
| **SN** | **Orthopaedic items with specifications** | **Price/Unit**  **(Rs)** |
|  | **Screw drivers** | |
|  | Torque limiting hexagonal screw driver QC handle, AO, 2.0 mm tip, 0.8 NM, 150 mm with markings |  |
|  | Torque limiting hexagonal screw driver QC handle, AO, 2.5 mm tip, 1.5 NM, 150 mm with markings |  |
|  | Screw driver QC shaft set of three (for 1.5, 2.4/2.7, 3.5/4.0 mm screws with markings) |  |
|  | Plain fibre handle hexagonal screw driver for 2.0 mm screw (Hex 1.5 mm) |  |
|  | **Wire cutter** | |
|  | Wire cutter with TC insert (Golden handle), 12” |  |
|  | Wire cutter, plier and bender combined, 9” |  |
|  | **Bone forceps & clamps** | |
|  | Condylar bone holding forceps ball pointed, ratchet lock, 8” |  |
|  | Ferguson bone holding forceps, 6.5 inch |  |
|  | Ferguson bone holding forceps, 8.0 inch |  |
|  | Reduction Forceps Pointed Jaw, speed lock, 6” |  |
|  | Kern/Lane Bone Holding Forceps, 6” |  |
|  | Kern/Lane Bone Holding Forceps, 8” |  |
|  | Small O’Brien Bone Clamp with Integrated drill guide andbone diameter gauge calibrated from 8mm to 30mm (Drill Guide Diameter: 8mm to accommodate up to 4mm screw): 6" |  |
|  | Extra small O’Brien Bone Clamp with Integrated drill guide and  bone diameter gauge: 4" |  |
|  | **Retractors** | |
|  | Alm microsurgical retractor, 4X4 prongs, 4” |  |
|  | Hohmann retractor 6 x 150 mm |  |
|  | Hohmann retractor 8 x 150 mm |  |
|  | Hohmann retractor 10 x 150 mm |  |
|  | Hohmann retractor 12 x 150 mm |  |
|  | Hohmann retractor 15 x 150 mm |  |
|  | Gelpi retractor, 6” |  |
|  | Mastoid retractor 4X5 prongs with blunt edges, 6” |  |
|  | Nerve root retractor, small, ~6” long |  |
|  | Senn retractor, small blunt, ~6” long |  |
|  | **Periosteal elevators** | |
|  | Mini Periosteal Elevator with straight edge |  |
|  | Periosteal Elevator with fibre handle, 3.0mm Width, Curved Blade, Straight Edge |  |
|  | Periosteal elevator with fibre handle, 6 mm width straight blade |  |
|  | Periosteal elevator with fibre handle, 8 mm width straight blade |  |
|  | Periosteal elevator with fibre handle, 10 mm width straight blade |  |
|  | **Rongeurs and punch** | |
|  | Kerrison Rongeurs, ~8”long, 3 mm edges |  |
|  | IVD Rongeurs, ~ 7”long, grasp 2X10 mm |  |
|  | IVD Rongeurs, ~ 7”long, grasp 3X10 mm |  |
|  | Toothed Leksell Bone Rongeurs, curved, ~9”long, 8mm edges |  |
|  | Toothed Leksell Bone Rongeurs, curved, ~9”long, 4mm edges |  |
|  | Kerrison Bone Punch, up cutting, 45X3 mm cutting |  |
|  | Kerrison Bone Punch, down cutting, 45X3 mm cutting |  |
|  | Kerrison Bone Punch 45x5 mm cutting |  |
|  | **Wire saw** | |
|  | Gigli saw handle set of 2 |  |
|  | Gigli saw wire, Pack of 25 |  |
|  | **Plate benders** | |
|  | Double slotted Mini and Small bone plate bender pair for 2.7 and 3.5 mm plates, 7” |  |
|  | Plate bending template small and medium |  |
|  | **Screw depth gauge** | |
|  | Mini Depth gauge, measuring length up to 30 mm |  |
|  | Small Depth gauge, measuring length up to 50 mm |  |
|  | **Taps related** | |
|  | QC tap for 2.7 mm cortical screw |  |
|  | QC tap for 3.5 mm cortical screw |  |
|  | QC tap for 4.0 mm cancellous screws |  |
|  | Bone tap handle for QC tipped taps for 2.7 to 4 mm screws taps |  |
|  | **Ortho wire related** | |
|  | Cerclage wire twister, 7” |  |
|  | Parallel wire guide 4 mm |  |
|  | Wire passer with fibre handle, mini |  |
|  | **Misc** | |
|  | LCP drill guide set of 4 (1.5/2.0, 1.8/2.4, 2.0/2.7 and 2.8/3.5 with markings and colour coding) |  |
|  | LCP Threaded Drill Guide Locking Screw Drill Guider 1pcs Veterinary Orthopedic Surgical Instruments |  |
|  | Diameter measuring combined scale for K-wire, screws, pins, drill bits and nails |  |
|  | Screw-washer hanger |  |
|  | SS Frazier suction tips, 2.0 mm |  |
|  | SS Frazier suction tips, 3.0 mm |  |
|  | SS Frazier suction tips, 4.0 mm |  |
|  | K-wire Introducer |  |
|  | K-wire tube, 8” |  |
|  | Bone hammer with fiber handle |  |
|  | Counter Sink (Separate QC handle and shaft set for 2.0, 2.7, 3.5 mm Screws) |  |
|  | Mini ocannulated SS Jacob’s Chuck with T Handle and 2 keys |  |
|  | Olsen Needle Holder and Scissors-Tungsten Carbide Tip, 6” |  |
|  | Olsen Needle Holder and Scissors-Tungsten Carbide Tip, 8” |  |
|  | Tudor Edwards Rib Shear, 8” |  |
|  | Penfield dissector set of 5, ~8”long, 3/4/7.5 mm edges |  |
|  | Inge lamina spreader, small, ~6” long |  |
|  | Sharp nerve hook |  |
|  | **Customized orthopaedic screw box (~12X7 inch) with accessories as per following details-**  Autoclavable sturdy Aluminium orthopaedic screw box with screw rack **as per attached design (Annexure 2)**. With sturdy locking mechanism as shown in the picture. The screw rack having laser markings and holes to accommodate-   1. 3.5 mm Cortical Screws (8-50 mm with 2 mm difference, 10-30 mm lengths in double rows), 4 screws in each row: **Total 132 screws** 2. 3.5 mm Locking Cortical Screws (8-50 mm with 2 mm difference, 10-30 mm lengths in double rows), 4 screws in each row: **Total 132 screws** 3. 3.5 mm Cancellous Screws (14-50 mm with 2 mm difference up to 40 mm and 5 mm difference thereafter), 2 screws in each row: **Total 32 screws** 4. 3.5 mm Locking Cancellous Screws (14-50 mm with 2 mm difference up to 40 mm and 5 mm difference thereafter), 2 screws in each row: **Total 32 screws** 5. 4.0 mm Cancellous Screws (14-50 mm with 2 mm difference up to 40 mm and 5 mm difference thereafter), 2 screws in each row: **Total 32 screws** 6. 4.0 mm locking cancellous Screws (14-50 mm with 2 mm difference up to 40 mm and 5 mm difference thereafter), 2 screws in each row: **Total 32 screws**   Screw length measuring gauge with 0-100 mm marking on one side of the rack; The markings of the name and lengths of screws on rack as per design; The outer side of the screw box lid with marking “**3.5 plain and locking cortical screws plus 3.5 and 4.0 mm plain and locking cancellous screw box**”  Screw forceps, 4 anti-skid drill bits (two each of 2.5, 2.7 mm size with size markings on shaft), 4 Threaded tip 1.5 mm, 150 mm K wire; 2.5 mm tip, 1.5 NM, torque control screw driver, 150 mm in silicon pad underneath the top rack.  **The screw box complete with all above-mentioned accessories including SS orthopaedic screws (Total nos.: 392)** |  |

|  |  |  |
| --- | --- | --- |
| **Applicable rate of GST** | **GST\*** | **Item nos.** |
| **5%** |  |
| **12%** |  |
| **18%** |  |
| **28%** |  |
| **Name and address of the bidding firm** |  | |
| **Telephone no.** |  | |
| **GST no.** |  | |

\*Kindly tick whatever applicable

**Signature of the bidder with name**

***Annexure 2***

****